**CLASSES:**

1. 7800- (Special) (Max Tire 18.4.38) (330ci max)(3200rpm)
2. 10000 (Special) (18 mph Pace)
3. 11500 (special)

**RULES AND REGULATIONS**

1. Farm tractors only, as is from the factory.
2. Driver pulls at his own risk. Safety equipment is required.
3. Driver must be 16 years of age. Those under 18 must have written permission.
4. Entry fee will be paid at the time of registration.
5. Weights must not be more than 24 in. in front of the tractor.
6. Drivers must remain seated while pulling or face disqualification.
7. Judges’ decisions are final.
8. Judges have the right to disqualify a tractor or driver for any rule violation.
9. Drawbar must be no more than 20 in. from the ground.
10. Drawbar must be a minimum of 18 in. from the center of the rear wheel to the point of hook-up.
11. Solid drawbar hook-up is mandatory. No hook-ups to 3-point or quick hitch.
12. Shifting is allowed, but the forward motion of the sled must not stop.
13. Hood, fuel tank, and fenders must remain in the proper place for safety.
14. The pull will start with a tight hook-up. No jerk starts.
15. Driver is weighed with the tractor. Any alterations after you are officially weighed in will be cause for disqualification.
16. Weights must not interfere with hook-up to sled.
17. Driver is disqualified if anything falls from the tractor during the pull.
18. Driver is disqualified if the tractor goes out of bounds.
19. Driver will be disqualified for reckless driving.
20. No alcoholic beverages allowed. Any driver appearing intoxicated will not be allowed to pull.
21. No entry refunds for disqualifications.
22. No alcohol or water injection except for Special or Hot Farm class.
23. Each puller must furnish its own clevis.
24. Tractors with slipper clutches may run Special or Hot Farm Classes only.
25. All tractors in Hot Farm & Special classes must have wide front ends.
26. All tractors in Hot Farm & Special classes- diesel must have air shut-offs and gas must have kill switches.
27. (All must be working)
28. All Hot Farm & Special classes must have wheelie skids extending 5 to 6 inches behind the rear wheels and 6 inches above the ground.
29. Special, Altered, & Hot Farm Tractors are not allowed in Farm classes

**Other Special Class Rules**

* 1. Max. 20.8.42 tires in Special class (Except 7800 – Max is 18.4.38)
  2. Max. 3000 RPMs. (Except 7800 which is 3200 RPMs)