6500 LB Street- Gas

Must be street(able)- able to drive down the road without rear wheels popping off road.

NO gutted cabs.

Naturally aspirated; Turbos only if it is OEM

NO Dominator Carburetors- 4150 base only

NO sanctioned trucks – open stock, superstock etc.

Must have mufflers, glass packs, etc. behind cab

NO solid suspension, not even extremely thick-thick springs that barely move. 1” of suspension travel minimum.

NO block suspension

NO weight bars, excessive homemade bumpers, or heavy push bars or brush guards.

ONLY DOT tires up to 35”

NO electric over hydraulic steering- OEM Gearbox with steering shaft, work power steering pump, belt driven.

NO modified frames – safety factor

NO bigger than 1 ton drivetrain

OEM heads

NO dry sump setups

NO electric water pumps- must have water pump, alternator, and power steering pump belt driven

NO hanging weights. If they are visible- hanging, they go in the bed or passengers side floor.

License and Insurance are encouraged

Safety equipment is strongly encouraged

Reese style hitch

If you do not meet these requirements you can pull with the Outlaw Class.

If we have enough registrations of small block and big block, we will separate the classes.