6000 Open Class

Tires: 18.4X38 top cut tires

Hitch: 20”

All safety equipment encouraged

8600 | 12 MPH Class

Tires: 18.4.38 top cut tires radial or bias

Hitch: 20”

Any fuel system: Diesel, Gas or LP

Required Safety Equipment:

Wheelie bards

Wide front

Air shut-off or kill switch